### M3A-ABS 40

Case: Black plastic Transparent plastic Quadrant: White plastic

Element gauges: Bourdon tube in copper alloy, solder alloy of tin

\_ C 60 bar spring,

\_ 60 bar spring curl Movement: Brass Specifications


Reference standards: EN 837-1 Pressure: Static: 75% of full scale Floating: 60% of full scale

For short periods: up to full scale Temperature Limits: Ambient: -20 ... +60 ° C Fluid: +60 ° C maximum

Storage: -20 ... +60 ° C

Thermal drift: ± 0.04% / 1K compared to (+20 ° C) Accuracy class: cl. 2.5, cl. 1.6 to request

Degree of protection: IP 31 to EN 60 529 / IEC 529

*Individual weight: 0,048 kg *